**GREEN LIFE GROUP  
 Technical Data Sheet**

**GEEN UP RC - RUBBER CLEANER**

**Description  
  
Green Up RC** is a powerful non chlorinated biodegradable water based  rubber  cleaner.  **Green-Up RC** liquid is high quality cleaning, removes and absorbs fats on the basis of water. **Green-Up RC** is a powerful non chlorinated cleaner for the cleaning of metallic surfaces special for heat transfer systems. Does not damage, plastic, metal or stainless steel surfaces **Green-Up RC** Prevents cleaning ability high fat and soot removing thin layers of rubber **Green-Up RC** is designed for industrial use in factories, fleets, garages. **Green-Up  RC**based on the 'green' components. Product convenient and comfortable to use, safe use, is non-flammable

**Green-Up  RC** is worker and environmentally friendly. Not contains harsh or hazardous ingredients. **Green-Up  RC** product is a special version optimized for this application. **Green-Up  RC** is not harm the environment

**Summary of Benefits**

* FOOD SAFE
* WATER BASED  CLEANER
* NOT DANGEROUS FOR PEOPLE
* NOT HURM THE INVIROMENT
* NON TAINTING
* NON FLAMMABLE
* DOES NOT DISCHARGE TOXIC GAS OR SYNTHETICSSMELL
* DOES NOT RISK THE BREATHING WAY
* DOES NOT LEAVE MARKS ON SKIN ORSKIN
* DOES NOT ATTACKING THE SURFACE, INCLUDING PLASTICK  AND STAINLESS STEEL.
* MONEY SAVED

**GREEN LIFE GROUP  
 Technical Data Sheet**

**GEEN UP RC - RUBBER CLEANER**

**-2-**

**Applications**

Cleaning rubber manufacturing plants, tires and conveyor belt drive  
Cleaning tracks with oils, fuels and erosion of rubber.  
Cleaning facilities and equipment   used in roads construction.  
Cleaning surfaces where flocks of rubber tires toy, concrete surfaces and runways  
Application of the product can be done by spraying, dipping, brushing or bedwetting.  
Disperse the material sprayed or applied topically to the area of cleaning,  
After 2-3 minutes rubbing the area sprayed  
Wait 5-10 minutes for the next step of washing with water.  
The waiting times can be determined after a trial instead.  
Green-Up Rubber Remover can be used through floor scrubbing machines;  
the dilution rate would need to be established by trial and error, as all machines are different   
  **Precautions**For external use only not for food, is not toxic  
Do not swallow  
Avoid contact with eyes or skin material recommended protective eyewear and gloves.  
In case of contact with eyes or skin wash with lots of water  
In case of swallowing, drink water or milk and seek medical assistance  
Keep away from children  
Keep the contains locked in a shady close place  
Avoid exposing the liquid to extreme temperatures  
  **Component**NATURAL non caustic readily biodegradable water based components   
Blend of surfactants from natural sources  sequestrants, silicates and natural  solvent carrier.   
This product contains a mixture of ingredients which are food industry safe.  
Non of the components is made of neither animals.  
The liquid does not contains minerals fats, or fats produce from animals  
Green Life Group is against experiments in animals and does not include in its  
 products components from them. **GREEN LIFE GROUP  
 Technical Data Sheet**

**GEEN UP RC - RUBBER CLEANER**

**-3-**

**Safety Precautions**Do not ingest this product. Avoid contact with eyes. In case of eye contact, rinse well with a large quantity of clean water flush for a minimum of 15 minutes. In case of swallowing, drink a large amount of water or milk and seek medical attention. Keep away from children. Keep the container in a closed shaded area. Avoid exposure to extremely high temperature.  
  **PHYSICAL PROPERTIES**Appearance:                                      -  CLEAR COLOURLESS OR RED LIQUID  
pH @ 5% DILUTION                          -             10  
Density                                               -             1.1  
Flash Point                                         -           None

**Health and Safety**

For full Health and Safety data please refer to our specific MSDS Sheet, which is available upon request

 **Pack Sizes** 18lt and 205lt barrels, 1000 litter canister   
 

Green Life Group P.B. 12644 Ashdod Israel 77520 www.egreen up.com

Email grnlf01@walla.co.il Fax 972(0) 88565645 Tel 972(0)88565648